SIP .NET Class Library
SIP .NET Class Library
SIP .NET
Independentsoft.Sip.Sdp
Connection Class
Connection Properties
Address Property
AddressType Property
NetworkType Property
NumberOfAddresses Property
TimeToLive Property

# Connection Properties

The Connection type exposes the following members.

Properties

| Name | Description
--- | --- | ---
| Address | Gets or sets connection address. Typically the connection address will be a class-D IP multicast group address. If the session is not multicast, then the connection address contains the fully-qualified domain name or the unicast IP address.
| AddressType | Gets or sets type of address.
| NetworkType | Gets or sets type of network.
| NumberOfAddresses | Gets or sets number of addresses.
| TimeToLive | Gets or sets time to live (TTL) value. Sessions using an IP multicast connection address must also have a TTL value present in addition to the multicast address. The TTL and the Address together define the scope with which multicast packets sent in this conference will be sent. TTL values must be in the range 0-255.

Top
See Also

#### Reference

Connection Class
Independentsoft.Sip.Sdp Namespace

Copyright 2023 Independentsoft

Send comments on this topic to support@independentsoft.de