SIP .NET Class Library
SIP .NET Class Library
SIP .NET
Independentsoft.Sip.Sdp
Connection Class
Connection Properties
Address Property
AddressType Property
NetworkType Property
NumberOfAddresses Property
TimeToLive Property

# Connection TimeToLive Property

Gets or sets time to live (TTL) value. Sessions using an IP multicast connection address must also have a TTL value present in addition to the multicast address. The TTL and the Address together define the scope with which multicast packets sent in this conference will be sent. TTL values must be in the range 0-255.

Namespace: Independentsoft.Sip.Sdp
Assembly: Independentsoft.Sip (in Independentsoft.Sip.dll) Version: 1.0.700.17927
Syntax
C#
VB
Copy

    public int TimeToLive { get; set; }

    Public Property TimeToLive As Integer
    	Get
    	Set

#### Property Value

Type: Int32
See Also

#### Reference

Connection Class
Independentsoft.Sip.Sdp Namespace

Copyright 2023 Independentsoft

Send comments on this topic to support@independentsoft.de